

 *******************************************************************
 *                                                                 *
 *                    SRH-2D Version 3.6.2                         *
 *             Sedimentation-River-Hydraulics (SRH) Model          *
 *                                                                 *
 *        Technical Service Center,  Bureau of Reclamation         *
 *        Contact: Yong G. Lai, Ph.D., ylai@usbr.gov               *
 *                                                                 *
 *******************************************************************

 ==> Code Execution Year-Month-Date:  2024  1 16


 ************************************************************
 *          Summary of Input Parameters and Variables       *
 ************************************************************

 SRH MODULE USED:
      Flow-Only Modeling
      Temperature Module is not activated
      Bank Erosion Module is not activated
      Turbulence Model: Depth-averaged parabolic zero-equation model

 MESH SIZE INFO:
      Total number of cells:              20930
      Total number of mesh points:        17099
      Total number of faces:              38050
      Total number of boundary faces:       869
      NCLVT:                              75231
      Number of Mesh Blocks:                  1
      Mesh Type: Unstructured mesh - SMS-2DM format

 STEADY/UNSTEADY SIMULATION PARAMETERS:
      Unsteady Simulation: YES, it is unsteady
      Initial Condition:   New run from user specified initial condition
      Number of time steps (ntstep):                   -1
      Number of iterations within each time step:       3
      Tstart(s) DT(s) DT_CHAN(s) Total_simu_time(hr):    0.0000E+00   5.0000E+00   5.0000E+00   1.5000E+01
      Laminar kinematic viscosity:                       1.0000E-06
      Turbulent Parabolic Model Constant:                7.0000E-01

 MISCELLENEOUS PARAMETERS:

 INTERMEDIATE RESULT PRINTOUT CONTROL:


 ************************************************************
 *       End of Input Parameters and Variables Summary      *
 ************************************************************

 ==> Mesh Size Info over Solution Domain
     Minimum Mesh Cell Area (m^2)      =   5.574E-01
     Maximum Mesh Cell Area (m^2)      =   4.138E+03
     Total Solution Domain Area (m^2)  =   4.937E+06

 ==> Smallest Angle between Cell-to-Cell-Base-Vector and Face =   2.048E+01
     Located at Face=   21833;    Between two cells:   11930   11937

 ==> Informational Output (These cells are set as INACTIVE/CUT-AWAY):
     There are pressure cells whose ceiling is below bed; Number =     5

 ==> Total water volume (m3) at t=tstart:
     Within Model Domain =   1.2186E+07


 *****************************************************
 *   SIMULATION INFORMATION PRINT OUT                *
 *****************************************************

