MESH2D
NUM_MATERIALS_PER_ELEM 1 
BEGPARAMDEF
GM  "SRH-2D"
SI  0
DY  0
TU  "Time Step (sec)/Total Time (hours)"
TD  0  0
KEY  "Yong Lai"
GP 1 "Global" 1
GP_DEF  1 1 "Simulation_Description" 3 "SRH-2D Simulation"
GP_DEF  1 2 "Case_Name" 3 "case"
GP_DEF  1 3 "Solver_Selection" 4 "Flow"
GP_OPTS 1 3  "Flow" "Morphological_Analysis"
GP_DEF  1 4 "Steady_or_Unsteady" 4 "Steady"
GP_OPTS 1 4  "Steady" "Unsteady"
GP_DEF  1 5 "Start_Time(hours)" 2 0 0 1.79769e+308
GP_DEF  1 6 "Time_Step(seconds)" 2 1 0 1.79769e+308
GP_DEF  1 7 "Total_Simulation_Time(hours)" 2 1 0 1.79769e+308
GP_DEF  1 8 "Initial_Condition" 4 "Dry"
GP_OPTS 1 8  "Dry" "RST_File" "Automatic"
GP_DEF  1 9 "RST_File_Name" 3 "_RST.dat"
GP_DEP 1 9 "PARENT_SELF" "Initial_Condition" 0 "Dry" 0 "RST_File" 1 "Automatic" 0 
GP_DEF  1 10 "Mesh_Unit" 4 "Feet"
GP_OPTS 1 10  "Feet" "Meters" "Miles" "Inches" "Millimeters" "Kilometers"
GP 2 "Flow_Module" 1
GP_DEF  2 1 "Turbulence_Model" 4 "Zero_Equation"
GP_OPTS 2 1  "Zero_Equation" "KE_2_Equation"
GP_DEF  2 2 "A_Constant" 2 0.7 0.001 10
GP_DEP 2 2 "PARENT_SELF" "Turbulence_Model" 1 "Zero_Equation" 1 "KE_2_Equation" 0 
GP 3 "Output" 1
GP_DEF  3 1 "Result_Output_Format" 4 "XMDF"
GP_OPTS 3 1  "XMDF" "SRHN" "SRHC" "TECplot"
GP_DEF  3 2 "Result_Output_Unit" 4 "English"
GP_OPTS 3 2  "English" "SI"
GP_DEF  3 3 "Result_Output_Frequency(hours)" 2 -1 -1.1 1.79769e+308
NUME  3
BCPGC  1
DISP_OPTS entity   0 0 0 0 1 0 0 0
DISP_OPTS inactive 0 0 0 0 1 0 0 0
DISP_OPTS multiple 0 0 0 0 1 0 0 0
BEFONT  0 -11 0 0 0 400 0 0 0 0 3 2 3 18 "Arial"
BC  0 "Monitor Point" 1 0 1 "(none)"
BC_DISP_OPTS 1 0 0 0 0 1 0 1 1
DISP_OPTS entity   1 153 51 51 1 0 2 0
DISP_OPTS inactive 1 153 51 51 1 0 1 0
DISP_OPTS multiple 1 0 0 0 1 0 1 0
BEFONT  1 -11 0 0 0 400 0 0 0 0 3 2 3 18 "Arial"
BC  1 "Inlet-Q (subcritical inflow)" 1 0 1 "(none)"
BC_DEF 1 1 "Discharge(Q)" 4 "Constant"
BC_OPTS 1 1  "Constant" "Time_Series"
BC_DEF 1 2 "Constant_Q" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 2 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 1 "Time_Series" 0 
BC_DEF 1 3 "Time_Series_FileName" 3 ""
BC_DEP 1 3 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 0 "Time_Series" 1 
BC_DEF 1 4 "Unit_of_Q" 4 "cfs"
BC_OPTS 1 4  "cfs" "cms"
BC_DEP 1 4 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 1 "Time_Series" 0 
BC_DEF 1 5 "Unit_of_Time&Q" 4 "hours&cfs"
BC_OPTS 1 5  "hours&cfs" "hours&cms"
BC_DEP 1 5 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 0 "Time_Series" 1 
BC_DEF 1 6 "Distribution_at_Inlet" 4 "Conveyance"
BC_OPTS 1 6  "Conveyance" "Constant_Velocity" "Constant_q"
BC_DISP_OPTS 1 1 0 0 0 1 0 1 1
BC  1 "Exit-H (subcritical outflow)" 2 0 1 "(none)"
BC_DEF 2 1 "Water_Elevation(WSE)" 4 "Constant"
BC_OPTS 2 1  "Constant" "Time_Series" "Rating_Curve"
BC_DEF 2 2 "Constant_WSE_Value" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 2 2 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 1 "Time_Series" 0 "Rating_Curve" 0 
BC_DEF 2 3 "Time.vs.WSE_FileName" 3 ""
BC_DEP 2 3 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 1 "Rating_Curve" 0 
BC_DEF 2 4 "Q.vs.WSE_FileName" 3 ""
BC_DEP 2 4 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 0 "Rating_Curve" 1 
BC_DEF 2 5 "Unit_of_WSE" 4 "Feet"
BC_OPTS 2 5  "Feet" "Meters"
BC_DEP 2 5 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 1 "Time_Series" 0 "Rating_Curve" 0 
BC_DEF 2 6 "Unit_of_Time&WSE" 4 "hours&feet"
BC_OPTS 2 6  "hours&feet" "hours&meters"
BC_DEP 2 6 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 1 "Rating_Curve" 0 
BC_DEF 2 7 "Unit_of_Q&WSE" 4 "cfs&feet"
BC_OPTS 2 7  "cfs&feet" "cms&meters"
BC_DEP 2 7 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 0 "Rating_Curve" 1 
BC_DISP_OPTS 2 1 0 0 0 1 0 1 1
BC  1 "Exit-Q (known-Q outflow)" 3 0 1 "(none)"
BC_DEF 3 1 "Discharge(Q)" 4 "Constant"
BC_OPTS 3 1  "Constant" "Time_Series"
BC_DEF 3 2 "Constant_Q" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 2 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 1 "Time_Series" 0 
BC_DEF 3 3 "Time_Series_FileName" 3 ""
BC_DEP 3 3 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 0 "Time_Series" 1 
BC_DEF 3 4 "Unit_of_Q" 4 "cfs"
BC_OPTS 3 4  "cfs" "cms"
BC_DEP 3 4 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 1 "Time_Series" 0 
BC_DEF 3 5 "Unit_of_Time&Q" 4 "hours&cfs"
BC_OPTS 3 5  "hours&cfs" "hours&cms"
BC_DEP 3 5 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 0 "Time_Series" 1 
BC_DISP_OPTS 3 1 0 0 0 1 0 1 1
BC  1 "Inlet-SC (supercritical inflow)" 4 0 1 "(none)"
BC_DEF 4 1 "Discharge(Q)" 4 "Constant"
BC_OPTS 4 1  "Constant" "Time_Series"
BC_DEF 4 2 "Constant_Q" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 4 2 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 1 "Time_Series" 0 
BC_DEF 4 3 "Time_Series_FileName" 3 ""
BC_DEP 4 3 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 0 "Time_Series" 1 
BC_DEF 4 4 "Unit_of_Q" 4 "cfs"
BC_OPTS 4 4  "cfs" "cms"
BC_DEP 4 4 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 1 "Time_Series" 0 
BC_DEF 4 5 "Unit_of_Time&Q" 4 "hours&cfs"
BC_OPTS 4 5  "hours&cfs" "hours&cms"
BC_DEP 4 5 "PARENT_LOCAL" "Discharge(Q)" 1 "Constant" 0 "Time_Series" 1 
BC_DEF 4 6 "Water_Elevation(WSE)" 4 "Constant"
BC_OPTS 4 6  "Constant" "Time_Series" "Rating_Curve"
BC_DEF 4 7 "Constant_WSE_Value" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 4 7 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 1 "Time_Series" 0 "Rating_Curve" 0 
BC_DEF 4 8 "Time.vs.WSE_FileName" 3 ""
BC_DEP 4 8 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 1 "Rating_Curve" 0 
BC_DEF 4 9 "Q.vs.WSE_FileName" 3 ""
BC_DEP 4 9 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 0 "Rating_Curve" 1 
BC_DEF 4 10 "Unit_of_WSE" 4 "Feet"
BC_OPTS 4 10  "Feet" "Meters"
BC_DEP 4 10 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 1 "Time_Series" 0 "Rating_Curve" 0 
BC_DEF 4 11 "Unit_of_Time&WSE" 4 "hours&feet"
BC_OPTS 4 11  "hours&feet" "hours&meters"
BC_DEP 4 11 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 1 "Rating_Curve" 0 
BC_DEF 4 12 "Unit_of_Q&WSE" 4 "cfs&feet"
BC_OPTS 4 12  "cfs&feet" "cms&meters"
BC_DEP 4 12 "PARENT_LOCAL" "Water_Elevation(WSE)" 1 "Constant" 0 "Time_Series" 0 "Rating_Curve" 1 
BC_DEF 4 13 "Distribution_at_Inlet" 4 "Conveyance"
BC_OPTS 4 13  "Conveyance" "Constant_Velocity" "Constant_q"
BC_DISP_OPTS 4 1 0 0 0 1 0 1 1
BC  1 "Exit-EX (supercritical outflow)" 5 0 1 "(none)"
BC_DISP_OPTS 5 1 0 0 0 1 0 1 1
BC  1 "Exit-ND (normal-depth outflow)" 6 0 1 "(none)"
BC_DEF 6 1 "Discharge_Computed_at" 4 "Monitor-Line"
BC_OPTS 6 1  "Monitor-Line" "Inlet-Q#1"
BC_DEF 6 2 "Monitor_ID" 1 1 -100000 100000
BC_DEP 6 2 "PARENT_LOCAL" "Discharge_Computed_at" 1 "Monitor-Line" 1 "Inlet-Q#1" 0 
BC_DEF 6 3 "Bed_Slope" 2 0.001 0 0.9
BC_DISP_OPTS 6 1 0 0 0 1 0 1 1
BC  1 "Wall (No-slip boundary)" 7 0 1 "(none)"
BC_DISP_OPTS 7 1 0 0 0 1 0 1 1
BC  1 "Symmetry (Slip boundary)" 8 0 1 "(none)"
BC_DISP_OPTS 8 1 0 0 0 1 0 1 1
BC  1 "Monitor-Lines" 9 0 1 "(none)"
BC_DISP_OPTS 9 1 0 0 0 1 0 1 11
DISP_OPTS entity   2 0 0 0 1 0 0 0
DISP_OPTS inactive 2 0 0 0 1 0 1 0
DISP_OPTS multiple 2 0 0 0 1 0 1 0
BEFONT  2 -11 0 0 0 400 0 0 0 0 3 2 3 18 "Arial"
MAT_MULTI 0
MAT_DEF 2 1 "Manning's Roughness Coefficient" 2 0.02 0 10
ENDPARAMDEF
BEG2DMBC
END2DMBC
